IBM Spectrum Archive Single Drive Edition for Windows Version 2.4.5

(C) Copyright IBM Corporation 2010, 2022  All Rights Reserved

US Government Users Restricted Rights - Use, duplication or
disclosure restricted by GSA ADP Schedule Contract with
IBM Corp.
                ----------------------------------


Online user's guidance:
=======================
Before installing IBM Spectrum Archive on your system, refer to the information in the
online IBM Spectrum Archive Single Drive Edition documentation.

The online IBM Spectrum Archive Single Drive Edition documentation is available on the IBM Documentation:
  https://www.ibm.com/docs/en/spectrum-archive-sde

System Requirements:
====================
Supported Operating Systems:
    - Windows Server 2016
    - Windows 10

Supported Drives:
    - TS2380 IBM Tape drive
    - TS2370 IBM Tape drive
    - TS2360 IBM Tape drive
    - TS2350 IBM Tape drive
    - TS2290 IBM Tape drive
    - TS2280 IBM Tape drive
    - TS2270 IBM Tape drive
    - TS2260 IBM Tape drive
    - TS2250 IBM Tape drive
    - IBM 7226 Multimedia Storage Enclosure
    - TS1140 Enterprise Drive
    - TS1150 Enterprise Drive
    - TS1155 Enterprise Drive
    - TS1160 Enterprise Drive

For information about connectivity and supported configurations for the LTFS Spectrum Archive Single Drive Edition,
refer to the online IBM Spectrum Archive Single Drive Edition documentation available on the IBM Documentation:
     https://www.ibm.com/docs/en/spectrum-archive-sde

For information about supported versions of library and drive firmware,
and hardware interoperability known issues and limitations, refer to the IBM System Storage Interoperation Center (SSIC).

THE IBM SSIC can be found at the following website:
  http://www.ibm.com/systems/support/storage/config/ssic


Installing IBM Spectrum Archive:
================================

  Attention:
  If you are using an older version of LTFS or older version of IBM Spectrum Archive, uninstall it and restart your system before installing the new version of IBM Spectrum Archive.

  - Open Windows Explorer and double-click the .exe file that was downloaded
    in advance from the IBM FixCentral website.

  - Be sure to restart the system after installing IBM Spectrum Archive.

  - From the taskbar on the Windows desktop, open the "Configuration" panel.
    The Configuration panel allows the user to assign a drive letter for each
    LTFS-supported tape drive. After assigning a drive letter, the user can then
    access the tape drive as a file system.



Uninstalling IBM Spectrum Archive:
==================

  Attention:
  Eject media from the LTO drives before uninstalling IBM Spectrum Archive to avoid losing
  data in the cache.

  - Open the control panel and click "Uninstall a program" under "Programs."
    Then, right click "IBM Spectrum Archive Single Drive Edtion" and select "Uninstall."

  - Be sure to restart the system after uninstalling IBM Spectrum Archive.
